

 ***************************************************
 * Please read these instructions to find out      *
 * which file you should use during the upgrade.   *
 *                                                 *
 * There are two updates method (Method A &        *
 * Method B) if upgrading from earlier than        *
 * 12202.26.1.07H then use Method A. If upgrading  *
 * from 12202.26.1.07H or later then use Method B. *
 *                                                 *
 * eg                                              *
 * 12202.26.1.07    - Method A                     *
 * 12202.26.1.07a-g - Method A                     *
 * 12202.26.1.09    - Method B                     *
 ***************************************************

METHOD A - If upgrading from EARLIER than 12202.26.1.07H (eg 12202.26.1.07)
---------------------------------------------------------------------------
Ensure that power to the device is not interrupted during an upgrade or the unit could be rendered inoperable 

The firmware MUST be upgraded in the following sequence.

Step A. Upgrade to 12202.26.1.07H_1FULL.img via upgrade utility
Step B. Upgrade to 12202.26.1.10_FULL.img via upgrade utility

The full process is below:

1. Setup your computer to a static IP Address 

IP address: 192.168.1.5
Subnet Mask: 255.255.255.0 
Gateway: 192.168.1.1

2. Turn on the VigorPhone 350 on while pressing the ENTER and MENU buttons simultaneously.

3. The LCD on VigorPhone 350 will show “AUTO UPGRADE Wait for Image”

4. Load firmware upgade utility 

5. Manually enter 192.168.1.2 in Router IP field (do not click "..." button)

6. In Firmware file select 12202.26.1.07H_1FULL.img

7. Click Send

8. The firmware upgrade utility will send the file into the VigorPhone and the LCD display will show "AUTO UPGRADE...."

9. When complete the LCD will display "AUTO UPGRADE Upgrade Successful boot"

10. After the VigorPHone 350 has rebooted, press "Menu" > "6" > "select" > "4" > "select" and verify that the firmware shows 12202.26.1.07H_1

11. Repeat steps 2-10 with 12202.26.1.10_FULL.img

12. Press "Menu" > "6" > "select" > "4" > "select" and verify that the firmware shows 12202.26.1.08


Method B - If upgading from 12202.26.1.07H or later
---------------------------------------------------
Ensure that power to the device is not interrupted during an upgrade or the unit could be rendered inoperable 

1. Log into the VigorPhone Web UI

2. Go to System Settings > Firmware Upgrade

3. Choose 12202.26.1.10.img and click OK

4. The Web UI will display Upgrade Firmware and a upgade progress

5. Once complete the unit will automatically reboot



Further details regarding the upgrade process are on
http://www.draytek.co.uk/support/ippbx/kb_ippbx_VigorPhone_Upgrade.html