***********************************************************************************

    Release Notes for VigorPhone 350
    Firmware Version	: 12202.26.1.10
    Release Date        : 18th July 2012
    Applicable Models   : VigorPhone 350
    Locale              : UK ONLY

***********************************************************************************

*** IMPORTANT ****
Read the upgrade instructions (Upgrade_Instruction.txt) inclosed in this zip

[New Features]

1.  Users can configure the BLF button to support Line3 and Line4.

[Improvement]

1.  Fixed: Web UI compatibility problem with Google Chrome.
2.  Fixed: No audio issue when extension registered to VigorIPPBX3510 with PPTP and it receives call that is forwarded from SIP trunk
3.  Fixed: A noise occurs when a call is put hold with DrayTek Soft Phone.
4.  Fixed: Web UI compatibility problem with Internet Explorer 9
5.  Fixed: When there is an incoming call from SIP Trunk, DTMF cannot be detected if
someone dials the extension number.
6.  Fixed: Dialing to Hunt Group by using Vigor ATA-24, such call cannot be transferred by
IP Phone350.
7.  Fixed: When dialing the Voice Mail button with G729 only, the message of "please enter
your password" is distorted.
8.  Fixed: After restarting the second SIP registration and rebooting the device again, the
second account will be erased immediately.
9.  Improved: When there is a phone call coming from SIP Trunk, only the Caller Number
will be displayed. The Trunk number (eg *001) will not be displayed
10. Improved: Support Un-Attendant call transfer function.
11. Improved: Sporadic voice delay issue.
12. Improved: Answered calls list shows only the own number.
13. Improved: VigorPhone 350 cannot ring after the server sends the invite with
MIME-Version: 1.0 in message header.
14. Improved: VigorPhone 350 is unable to identify Subscription-State “terminated;
reason=timeout” when changing memory key function from BLF to Speed Dial.

[Known Issue]

1. Upgrading VigorPhone 350 to firmware version 12202.26.1.10 will cause device
configuration back to default settings. Please backup the System Configuration before
upgrading to 12202.26.1.10 and restore the file after the device successfully upgraded to
12202.26.1.10.
2. The old configuration file (earlier than 12202.26.1.07) is not compatible with the new
firmware.

***********************************************************************************

    Release Notes for VigorPhone 350
    Firmware Version	: 12202.26.1.09
    Release Date        : 8th November 2011
    Applicable Models   : VigorPhone 350
    Locale              : UK ONLY

***********************************************************************************


*** IMPORTANT ****
Read the Upgrade Instructions file (Upgrade  Instructions.txt) that is enclosed with this firmware.

If the firmware in the device is 12202.26.1.07 or earlier, please follow the steps as below
to upgrade the firmware,

Step1: 12202.26.1.07H_1FULL.img (via TFTP) (upgrade boot loader)
Step2: 12202.26.1.09_FULL.img (via TFTP) (upgrade firmware)

If the firmware in the device is 12202.26.1.07H or later, please upgrade it from Web
directly:
Step1: 12202.26.1.09.img (via Web) (upgrade firmware)


[New Features]

None

[Improvement]

1.  Resolved: Issue with transferring calls to a hunt group.
2.  Resolved: Unable to update correct BLF state for de-registered extensions.
3.  Resolved: Temporary Audio loss caused by re-registration of BLF status triggered by another VigorPhone350 going online.
4.  Resolved: If own BLF status changes, it could cause audio loss for other Vigor Phones
5.  Fixed: Unable to update correct BLF state for de-registered extensions.
6.  Improved: STUN server operation for SIP registration
7.  Improved: If display name and username are identical, then only one of them will be
displayed on display.
8.  Fixed: The handset microphone is still active when VigorPhone in speaker or headset mode. It might cause some echo or sound distortion.
9.  Fixed: Unable to successfully make an external call by pressing "Missed" menu button to
call.
10. Fixed: When the callee answers the call, the phone keeps ringing for 1 second.
11. Fixed: When using the BLF button first and then using the call park function later, the SIP
Accounts registration will be asked to perform again. VigorPhone 350 would loose SIP
registration and re-register immediately.
12. Fixed: When IPPBX transmits 200 OK packets to Phone350 again, it will not send ACK
packet back and cause to drop the call within 32 seconds.
13. Fixed: Time zone will be back to Taipei automatically (NTP time reverts from BST back
to GMT randomly)
14. Fixed: DTMF from VigorPhone350 can't be detected.
15. Fixed: If users select DHCP Client at the page LAN Port Settings, the Network Status
page of VigorPhone 350 won't display it correctly.
16. Fixed: The hunt group ID can't be saved after rebooting the device.
17. Improved: Export / import the configuration file of Phonebook and Speed Dial.
18. Improved: Add an audible warning when auto-answer is enabled.
19. Improved: Call forwarding can be quickly enabled / disabled via Advanced menu
20. Improved: Add Pick up function for Headset button
21. Improved: Add ring tone to remind users that line 2 is still online while hanging up line 1.
22. Improved: Add a user configurable option so that the user can choose if call waiting beep
function is enabled or disabled. If disabled, the 2nd call will receive busy reply.
(Phone Settings>>Other Settings>>Call Waiting)
23. Improved: The missed call counter only applies if the call is a direct call to the extension
and does not apply if the call is a call to a hunt group. (SIP Account>>Hunt Group)
24. Improved: Improve the display format of “missed calls” and “date”. The "x missed calls"
indication is too large. It makes the date disappeared and is disliked by users.
25. Improved: Missed call information can be enabled / disabled via Phone Settings > Other Settings
26. Improved: Default volume of wav1 is reduced slightly
27. Improved: Default microphone volume increased
28. Improved: “ #” or “*” can be added as dial digit.
29. Improved: "Handset Gain" (High / Low) setting added to volume controls. Set to High if the handset is too quiet.

[Known Issue]
1.  Upgrading VigorPhone 350 using the _FULL file will reset the device to factory defaults. 

***********************************************************************************

    Release Notes for VigorPhone 350
    Firmware Version	: 12202.26.1.08 
    Release Date        : 11th Octover 2011
    Applicable Models   : VigorPhone 350
    Locale              : UK ONLY

***********************************************************************************

[New Features]
1. Hold Reminder tones indicate that a call is on hold.
2. User is able to Transfer call #2 while call #1 is on hold
3. Call waiting function can be disabled / enabled
4. Missed call display can be disabled / enabled
5. Calls to hunt groups can be ignored for the purposes of missed call recording. The list of hunt groups that should not trigger a missed call is set via SIP Account Settings
6. Pressing DND will send Busy notification to IPPBX (PBX needs to be on 3.5.6 firmware)
7. Once configured "Always Forward" can be quickly disabled / enabled via the Adv menu on display

[Improvements & Corrected Problems]
1. Default handset / headset volume has been increased
2. Missed Call text moved so that it does not obscure the date
3. After user hangs up the phone will commence audible ring for ringing calls that came in before the user had hung up first line
4. Date Display layout improved slightly
5. Resolves issue which would cause VigorPhone to cease sending re-registration SIP requests
6. Web UI Volume settings page fixed
7. Corrected issue that could cause audio to be lost mid call for 5 seconds
8. Fixed NTP issue where timezone would change to GMT instead of "London, Edinburgh"




***********************************************************************************

    Release Notes for VigorPhone 350
    Firmware Version	: 12202.26.1.07 (formal release)
    Release Date        : 3rd May 2011
    Applicable Models   : VigorPhone 350
    Locale              : UK ONLY

***********************************************************************************

For more UK product details & specification, please visit www.draytek.co.uk

For UK support, visit www.support.draytek.co.uk

[New Features]
1. Built-in PPTP VPN Added. This can be setup through the 'Network' > 'VPN Setting' menu 
2. Intercom function can be disabled / enabled via Web Ui

[Improvements & Corrected Problems]
1.  User can not accidentially scroll to a SIP Account profile that is disabled.
2.  Changing the gain value in Web UI Voice Settings menu affects volume levels
3.  Displayed time would not change to Daylight saving at certain times of the year
4.  Auto-provisioning error if VigorIPPBX HTTP port was changed from port 80
5.  Decreases minimum volume level to a lower value compared to minimum volume level on previous firmware
6.  Call Transfer compatability improvements relating to the to-tag and from-tag usage
7.  Added ability to Reject 2nd call if user is currently on a call
8.  Spelling correction for "Temporarily unavailable" message in LED display   

[Known Issue]

***********************************************************************************

    Release Notes for VigorPhone 350
    Firmware Version	: 12202.26.1.06 (formal release)
    Release Date        : 4th October 2010
    Build Date	        : 17th September 2010
    Applicable Models   : VigorPhone 350
    Locale              : UK ONLY

***********************************************************************************

For more UK product details & specification, please visit www.draytek.co.uk

For UK support, visit www.support.draytek.co.uk

[Improvements & Corrected Problems]
1. Fixed: In some circumstances VigorPhone 350 used wrong codec for RTP, and Codec Negotiation Behavior changes on 200 OK with SDP (SIP stack)
2. Fixed: VigorPhone 350 uses the "to tag" information of 200 OK.
3. Fixed: In some circumstances VigorPhone 350 would stop ringing and not send "CANCEL" to let the caller know that the call has been rejected.
4. Fixed: When press the "reject" button, VigorPhone 350 will send "487 cancel" not "486 busy". Changed to "486 busy" so that IPPBX "on busy" action is followed/
5. Fixed: VigorPhone 350 sends duplicated notify requests to IPPBX when the BLF function is enabled.
6. Added: Beep call waiting notification to indication a second incoming call.

[Known Issue]
1. Upgrading VigorPhone 350 to firmware version 12202.26.1.06 will reset the device configuration to default. Please backup the System Configuration before upgrading to 12202.26.1.06
and restore the file after the device successfully upgraded to 12202.26.1.06.

[Notes]
1. If the firmware of the device is 12202.26.1.03 or earlier, please upgrade the VigorPhone 350 to
12202.26.1.04 before performing device firmware upgrade to 12202.26.1.06.


***********************************************************************************

    Release Notes for VigorPhone 350
    Firmware Version	: 12202.26.1.05 (formal release)
    Release Date        : 18th June 2010
    Build Date	        : 10th June 2010
    Applicable Models   : VigorPhone 350
    Locale              : UK ONLY

***********************************************************************************

New Features
1. Add ptime attribute in SIP Session Description Protocol (SDP).
2. Allow two different domain accounts set in PhoneBook to dial each other
3. Add rport parameter in SIP Via header field


Improvement
1. Fixed: STUN issue.
2. Fixed: Abnormal month display. When “auto” is selected for daylight saving in NTP&Time setting, more than 12 selections (months) will be offered for Start and End Month items.
3. Fixed: Wrong display of caller ID in LCM of VigorPhone 350 after performing call transfer.
4. Fixed: VigorPhone 350 jitter issue causes bad voice quality.
5. Fixed: Ring tone problem. There are three types of default ring tone for choosing.
6. Fixed: Incorrect time display for daylight saving.
7. Improved: VigorPhone has registered to VigorIPPBX 2820. After finishing the registration, the
user continues to dial local telephone. When the remote end picks up the phone call, the user
stills hears the ringing tone from VigorPhone. Later, VigorIPPBX 2820 sends the re-inviting to
the remote end, VigorPhone will response with “destination unreachable”.
8. Improved: A problem occurs when many characters are entered in the field of “Registration Server” and are saved in VigorPhone 350.


***********************************************************************************

    Release Notes for VigorPhone 350
    Firmware Version	: 12202.26.1.04 (formal release)
    Release Date        : 9th June 2010
    Build Date	        : 2nd June 2010
    Applicable Models   : VigorPhone 350
    Locale              : UK ONLY

***********************************************************************************

[New Features]
1. Added TFTP server facility to update and restore the firmware


***********************************************************************************

    Release Notes for VigorPhone 350
    Firmware Version	: 12202.26.1.03 (initial release)
    Release Date        : 21st September 2009
    Build Date	        : 10th September 2009
    Applicable Models   : VigorPhone 350
    Locale              : UK ONLY

***********************************************************************************

 - Initial Release firmware
