Vigor Router2200USB (UK Issue)

Build Date  : Mon Oct 13 9:21:58.76 
F/W Version : 2.3.7 (For UK Only)
Status      : Formal Release

Release Note
------------

Note : You should use V 2.5.2 (or later) router tools. If you
are upgrading from much older firmware (e.g. 2.3.2 or earlier)
you should upgrade using the .RST file, instead of the .ALL file.
The .RST file will clear out all of your existing settings (but
not the USB modem firmware, so that will remain).

1. New Features

- Support for USB Printers (Epsom, Brother, HP Tested)
  Printer support is ui-directional, so you cannot use printer
  PC utilities or multi-function devices (scanners etc.)
- New code to allow for BTOpenworld HG changes
- VigorCam support

----------------------------------
        
Build Date  : Wed 15 Jan 2003  18:58
F/W Version : 2.3.1
Status      : Formal Release

Release Note

1. New Features

    - Support MPoA (Multiple Protocols Over AAL5)
    - Can use fix IP to establish a PPP connection
    - Can detect VPI/VCI/Encapsulation/Protocol automatically
    - Add Telnet command "usb erase" to clean up USB modem 
      firmware stored in flash memory
    - Supports Alcatel Speedtouch330 and BT Voyager (not Voyager100) USB modems
    - Improved handling for UDP fragmentation (caused problems with games)
    - Webcam supported (currently Vigorcam supported only, when released)

2. Fixed Issues

    - When syslog function is enabled, router could sometimes hang 
      when dropping a PPP connection from the Web configurator.
    - VPN passthrough didn't work for some software clients
    - Improved VPN performance 
    - DDNS activity could cause DDNS server clash

3. Router Tools

   - Firmware upgrade utility changed to allow password entry for
     older firmware versions during upgrade.


For latest updates, please visit :

http://www.support.draytek.co.uk
