*************************************************
Release Notes for Vigor3100 series

	Firmware Version : 2.8.3 - Formal Release
	Release Date 	 : 4th Feb, 2010
	Build Date 	 : 28th Oct, 2009
	Applied Models 	 : Vigor3100, Vigor3120
	Locale		 : UK / Ireland

*************************************************

[New Features]
1. Add a new SHDSL driver R4.3 (recommended for France).
2. Add auto rebooting schedule.
3. Support more 3.5G modems which will be listed on DrayTek web site.

[Improvement]
1. Improved: VPN routing function.
2. Fixed: Configuration Restore would not work with configuration file from older firmware
3. Corrected: DHCP server gives out invalid IPs.




*************************************************
Release Notes for Vigor3100 series

Firmware Version : 2.8.2.1
Release Date : December 12, 2008
Applied Models : Vigor3100, Vigor3120

*************************************************

[New Functions] 
1. Add telnet command \"Srv nat ipsecpass\" for IPSec NAT passthrough. 
2. Add WAN interface in static route web page. 
3. Support PPPoA bridge function. 
4. Support Bandwidth Limit function for 2nd subnet. 
5. Support TFTP ALG. 
6. Support more 3.5G modems(C-Motech D-50, CDU-550, Sierra 875U, ASUS T500 and 
OVATION MC950D).

[Improvements] 
1. Remove limitation of PPTP HOST-To-LAN can only set up 16 VPN connections. 
2. Update CPA URL
3. Improve DHCP function. 
4. Set the default WAN detection mode of MPoA as ARP detection. 


*************************************************
Release Notes for Vigor3100 series

Firmware Version : 2.8.1
Release Date : January 2, 2008

Applied Models : Vigor3100, Vigor3120

*************************************************
[New Features]

[Improvements & Corrected Problems] 
- Improve compatibility with Windows Vista.

*************************************************
Release Notes for Vigor3100 series

Firmware Version : 2.8
Release Date : August 22, 2007

************************************************
[New Features]
- Support 3G USB Modem Backup.

************************************************

    Release Notes for Vigor3100 Series

    Firmware Version    : 2.7.1
    Release Date        : December 8, 2006

    Applied Models      : Vigor3100, Vigor3100G, Vigor3120
 
************************************************

[New Features]
- Suport 4-wire bundle mode on Vigor3120.

[Improvements & Corrected Problems] 
- Improve wireless 802.1X.
- Expand the length of Username and Password fields from 15 to 63 characters on Mail Alert Setup.


*************************************************
    Release Notes for Vigor3100 - UK Firmware/Version

    Firmware Version    : 2.7.0 UK 
    Release Date        : October 25, 2006
    Firmware build Date : Wed Sep 20 2006 19:41:33.21
    Applicable Models   : Vigor3100

*************************************************

[Release Firmware]
 - Update modem code from 3.0.5 to 3.0.8.1.


[New Features]
 - Support EOC packets and improve DSL interoperability.
 - Add "Traffic Graph" to show the session/bandwidth graph on WUI (Web User Interface).
 - Add "QoS Outbound TCP ACK Prioritize" to improve the download performance.


******************************************************************************************

    Firmware Version    : 2.6.0 UK (First Formal Release)
    Release Date        : November 16, 2005 
    Firmware build Date : Wed Nov 16 2005 09:12:46

******************************************************************************************

[Introduction]

The Vigor3100 family is compliance of G.SHDSL (ITU G.991.2).
The maximum bandwidth is up to 2.3Mbps for downstream and 2.3Mbps for upstream.
The Vigor3100 is not compatible with ADSL lines.

[Notes]
 - Back-to-back routing is not currently supported.

      
[End of File]
