**********************************************************************

    Release Notes for Vigor 3900
    Firmware Version    : 1.0.7.1 (Formal Release)
    Release Date        : 13th November 2013
    Build Date		: 12th November 2013
    Revision		: r3067
    Applicable Models   : Vigor 3900
    Locale              : UK ONLY
	
**********************************************************************

[New Features]
None.

[Improvement]
1.  Support USB-WAN for WAN Profile under the Setting tab in Application>> Dynamic DNS.
2.  Support WCF (web content filter) in High Availability (HA) application.
3.  Modify the mechanism for IP filter, "if no further match" action.
4.  Add a subnet mask setting, 255.255.255.254, for WAN IP configuration.
5.  Added option disable negotiation for Fiber WAN under the Interface tab in WAN>>Switch.
6.  ‘space’ special character can be used in the username for LDAP
7.  QoS IP rule can apply the packets passing through both Local IP and Remote IP.
8.  Improved PPTP service mechanism for multiple simultaneous LAN to LAN dial-ins
9.  Corrected: Can not block / unblock some IPs on Diagnostics>>Data Flow Monitor.
10. Corrected issue with ICMP packets larger than 8138 bytes over IPSec LAN to LAN tunnel.
11. Corrected: The user can not access Internet when QoS queue weight is set as “0”.
12. Corrected: Lower the priority of Inter-LAN routing function.
13. Corrected: LAN DHCP packets do not respond while LAN DHCP Server is OFF.
14. Corrected: Can’t accept L2TP VPN from none default route WAN.
15. Corrected: RADIUS client (Vigor router) sends wrong NAS IP address (127.0.0.1).
16. Corrected traffic status of DHCP over IPsec in VPN Connection Management.
17. ARP detection may fail when WAN TX traffic is full.
18. Corrected: SMS can't be sent out when L2TP over IPsec is up and down.

[Known Issue]
1.  VPN Trunk tunnel doesn't work well when the profile name is more than 15 characters.
2.  You need to disable "Force IPsec with L2TP" options for pure L2TP tunnel in [VPN and
Remote Access]>[PPP General Setup]

**********************************************************************

    Release Notes for Vigor 3900
    Firmware Version    : 1.0.7 (Formal Release)
	Revision			: 2733
    Release Date        : 2nd Sept 2013
    Build Date			: 27th Aug 2013
    Applicable Models   : Vigor 3900
    Locale              : UK ONLY
	
**********************************************************************

[New Features]
1.  Support Central VPN Management (CVM). Up to 16 devices can be managed.
2.  Support 3G backup/load balance.
3.  Support inbound load balance.
4.  Support VPN Trunk failover mode.
5.  Support PPPoE quota setting and MAC address filter.
6.  Support USB temperature sensor. http://www.draytek.co.uk/products/usb-thermometer.html
7.  Support SMS, Email Alert and Notification object profiles for WAN/VPN connection and USB temperature sensor.

[Improvements]
1.  Improved: Support SmartMonitor users up to 500.
2.  Improved: VPN Trunk throughput and stability.
3.  Improved: By default disable insecure SSL Encryption Key Algorithms
4.  Improved: Support DHCP relay on VPN.
5.  Improved: Add Active Standby mode for High Availability (HA).
6.  Improved: QoS redesigned
7.  Improved: Username reported to Syslog
8.  Improved: Add option 60(Vendor ID), 61(Client ID) for WAN DHCP mode.
9.  Improved: Add default maximum session number for Session limit.
10. Improved: Add flow control settings for Switch.
11. Improved: Add user defined options for DHCP server.
12. Improved: Improve DMZ function.
13. Improved: Add log and force update function for DDNS.
14. Improved: Add Force L2TP with IPsec policy option enabled in default.
15. Improved: Corrected causes for high CPU usage being displayed in Web UI
16. Improved: Stability in TR-069.
17. Improved: Firmware upgrade speed.
18. Fixed: Time object cannot work correctly when daylight saving is enabled.

[Known Issue]
1.  VPN Trunk tunnel doesn't work well when the profile name is more than 15 characters.
2.  You need to disable "Force IPsec with L2TP" options for pure L2TP tunnel in [VPN and
Remote Access]>[PPP General Setup]

**********************************************************************

    Release Notes for Vigor 3900
    Firmware Version    : 1.0.6.1 (Formal Release)
    Release Date        : 10th April 2013
    Build Date		: 25th March 2013
    Applicable Models   : Vigor 3900
    Locale              : UK ONLY

**********************************************************************

[New Features]
None

[Improvements]
1.  NAT Port Redirection Rule for FTP server didn't work with two WAN connection
2.  Customized web content message would disappear after rebooting the router
3.  Improvements to VPN Trunk tunnel where profile name are long
4.  PPTP connection display error in VPN Graph for syslog utility
5.  PPTP WAN could not dial-up if the server was set with a domain name
6.  Fixed issue with ping to VPN remote network working after clicking WAN DHCP Renew
Button via web user interface
7.  Fixed Session limit rule notapplying the correct limit due to subnet mask caculation error
8.  Fixed that WAN status displays “up” when the WAN cable is unplugged and WAN detect mode is set with “None”
9.  Corrected an issue with SNMP set/get Community setting
10. Resolved that VPN traffic wouldn't flow while one of the VPN GRE tunnels is disconnected
11. Corrected issue preventing some vLAN users from accessing Internet via Browser
12. Improved DHCP renewal interoperability
13. Fixed LAN VLAN configuration issues after restoring the web configuration
14. Corrected WAN1 MAC address used
15. Improved SIP ALG feature
16. Fixed that IPSec tunnel uptime would not reset after VPN reconnection
17. Corrected PPTP sessions problem that would prevent new network connections being setup
18. Corrected that a PC from remote subnet could't access Internet via PPTP LAN to LAN tunnel
19. Improvments to IPv6 traffic handling via AICCU
20. Improved load balance where multiple PPPoE connections have the same gateway
21. Corrected issue where multiple WAN disconnections could prevent VPN Trunk from reconnecting 
22. Added information for remote network connected with GRE over IPsec to Routing Table
23. Corrected issue where enabling Perfect Forward Secrecy in VPN client could prevent connection
24. Display issue with transmitted/received (TX/ RX) packets in Connection Management fixed for VPN clients behind NAT
25. Improved parameters stability for TR-069
26. Improved throughput between different VLANs
27. Added sending ARP for WAN Alias IP to WAN Gateway when connected
28. Added support for VPN on Alias WAN IP and IP Routing IP
29. Add mail alert when VPN is up
30. High availability improvements


[Known Issues]
1. VPN Trunk tunnel profile names should be kept to less than 15 characters.


**********************************************************************

    Release Notes for Vigor 3900
    Firmware Version    : 1.0.6 (Formal Release)
    Release Date        : 2nd Jan 2013
    Build Date		: 6th Nov 2012
    Applicable Models   : Vigor 3900
    Locale              : UK ONLY

**********************************************************************

[New Features]
1.  VPN(IPSEC) Routing Acceleration
2.  Supports PPPoE server for LAN PC connection
3.  Support VPN Alarm via E-mail & Syslog
4.  Support VPN Graph for syslog utility
5.  Support PPP mode for IPv6
6.  Support domain name for IPSec/PPTP dial-out

[Improvements]
1.  URL filter can block HTTPS connection by host keyword
2.  WCF support https block by web category
3.  Add QQ account filter for Firewall
4.  WAN4 is regarded as physical DMZ port
5.  Add time schedule for session limit and bandwidth limit
6.  Web content filter (WCF) stability improvements
7.  Data flow monitor resource allocation improvements
8.  DHCP server cannot work when Multi-LANs is configured
9.  Hosts under routing LAN can not access into the router
10. Configuration backup may fail
11. UPnP improved
12. Changing web port could prevent User management from working
13. WebUI server security improvements
14. IPsec RX/TX packets count may have error after entering phase2 rekey
15. L2TP connection status error after disconnection.
16  Cannot create IPsec VPN in aggressive mode when selecting AES as IKE phase 1
encryption.
17. PPTP dial-in may fail while using static IP mode.
18. VPN load balance may not work after connection reconnects
19. SSL Application doesn't work when HTTPS port is not set with 443.
20. Support PPTP dial on demand and idle timeout.
21. Support URL filter rules move up/down.
22. Support VLAN priority in LAN/WAN interface.
23. Support QoS packet by DiffServ (DSCP/TOS) for outgoing packet.
24. Let the user profile password support more special characters in standard
ASCII table.
25. Show the IP binding with MAC in DHCP table.
26. Mail Alert Send test e-mail button added
27. Add 36 regions time zone options for NTP.
28. Improve user management login process.
29. Add Common Name Identifier field in LDAP configuration.
30. Add an option for DDNS to select Internet IP or WAN IP.

[Known Issue]
1.  VPN Trunk tunnel profile names must be less than 15 characters.


**********************************************************************

    Release Notes for Vigor 3900
    Firmware Version    : 1.0.5 (Formal Release)
    Release Date        : 4th Sept 2012
    Applicable Models   : Vigor 3900
    Locale              : UK ONLY

**********************************************************************

First Firmware Release

[Known Issues]

- Devices on non-NAT subnets are unable to access the routers management interface

[END OF FILE]