**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.7.1 (Formal Release)
    Release Date        : 13th November 2013
    Build Date		: 12th November 2013
    Revision		: r3067
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[New Features]
None.

[Improvement]
1.  Support USB-WAN for WAN Profile under the Setting tab in Application>> Dynamic DNS.
2.  Modify the mechanism for IP filter, "if no further match" action.
3.  Add a subnet mask setting, 255.255.255.254, for WAN IP configuration.
4.  Added option disable negotiation for Fiber WAN under the Interface tab in WAN>>Switch.
5.  QoS IP rule can apply the packets passing through both Local IP and Remote IP.
6.  ‘space’ special character can be used in the username for LDAP
7.  Improved PPTP service mechanism for multiple simultaneous LAN to LAN dial-ins
8.  Corrected: Can not block / unblock some IPs on Diagnostics>>Data Flow Monitor.
9.  Corrected issue with ICMP packets larger than 8138 bytes over IPSec LAN to LAN tunnel.
10. Corrected: The user can not access Internet when QoS queue weight is set as “0”.
11. Corrected: Lower the priority of Inter-LAN routing function.
12. Corrected: LAN DHCP packets do not respond while LAN DHCP Server is OFF.
13. Corrected: Can’t accept L2TP VPN from none default route WAN.
14. Corrected: RADIUS client (Vigor router) sends wrong NAS IP address (127.0.0.1).
15. Corrected traffic status of DHCP over IPsec in VPN Connection Management.
16. ARP detection may fail when WAN TX traffic is full.
17. Corrected: SMS can't be sent out when L2TP over IPsec is up and down.

[Known Issue]
1.  VPN Trunk tunnel doesn't work well when the profile name is more than 15 characters.
2.  You need to disable "Force IPsec with L2TP" options for pure L2TP tunnel in [VPN and
Remote Access]>[PPP General Setup]

**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.7 (Formal Release)
    Build		: r2733
    Release Date        : 2nd Sept 2013
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[New Features]
1.  Support Central VPN Management (CVM). Up to 12 devices can be managed.
2.  Support 3G backup/load balance.
3.  Support inbound load balance.
4.  Support VPN Trunk failover mode.
5.  Support PPPoE quota setting and MAC address filter.
6.  Support USB temperature sensor. http://www.draytek.co.uk/products/usb-thermometer.html
7.  Support SMS, Email Alert and Notification object profiles for WAN/VPN connection and USB temperature sensor.
8.  Support Bridge VLAN function for LAN/WAN bridging.

[Improvement]
1.  Improved: Support SmartMonitor users up to 200.
2.  Improved: VPN Trunk throughput and stability.
3.  Improved: By default disable insecure SSL Encryption Key Algorithms
4.  Improved: Support DHCP relay on VPN.
5.  Improved: QoS redesigned
6.  Improved: Username reported to Syslog
7.  Improved: Add option 60(Vendor ID), 61(Client ID) for WAN DHCP mode.
8.  Improved: Add default maximum session number for Session limit.
9.  Improved: Add flow control settings for Switch.
10. Improved: Add user defined options for DHCP server.
11. Improved: Improve DMZ function.
12. Improved: Add log and force update function for DDNS.
13. Improved: Add Force L2TP with IPsec policy option enabled in default.
14. Improved: Corrected causes for high CPU usage being displayed in Web UI
15. Improved: Stability in TR-069.
16. Improved: Firmware upgrade speed.
17. Fixed: Time object cannot work correctly when daylight saving is enabled.

[Known Issue]
1.  VPN Trunk tunnel doesn't work well when the profile name is more than 15 characters.
2.  You need to disable "Force IPsec with L2TP" options for pure L2TP tunnel in [VPN and
Remote Access]>[PPP General Setup]

**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.6.2 (Formal Release)
    Build		: r2215
    Release Date        : 5th July 2013
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[New Features]
None

[Improvements]
1. Resolved LAN port inter-operability issue that could cause the Vigor 2960 to disconnect from the LAN after a period of time
2. WAN re-connection could trigger VPN trunk to disconnect

**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.6.1 (Formal Release)
    Release Date        : 26th April 2013
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[New Features]
None

[Improvements]
1.  Improved the throughput among different VLANs.
2.  Add support for VPN on Alias WAN IP and IP Routing IP.
3.  Send ARP of WAN Alias IP to WAN Gateway when connected.
4.  Configuration Backup menu improved
5.  Added more parameters and improved the stability for TR-069.
6.  NAT Port Redirection Rule for FTP server didn't work when two WAN
connections are up.
7.  Customized web content message disappears after rebooting the router.
8.  VPN Trunk tunnel didn't work well when the profile name was long.
9.  Corrected display error for PPTP connection in VPN Graph on Syslog.
10. Ping to VPN remote network didn't work after clicking WAN DHCP Renew
Button via web user interface.
11. Session limit applied the incorrect limit due to error in calculating mask.
12. WAN status was up while WAN cable was unplugged and WAN detection mode
was set to None.
13. Something wrong with SNMP Set/Get Community.
14. VPN Traffic could not pass anymore while one of the VPN GRE tunnels was
disconnected.
15. Corrected DHCP renew interoperability issue with some ISPs.
16. Corrected SIP ALG
17. IPSec tunnel uptime might not reset whene tunnel disconnected and re-established
18. Corrected issue with PPTP control session that could prevent new connections.
19. A PC from remote subnet via PPTP LAN to LAN couldn't access into Internet via VPN
20. Improved handling of certain IPv6 packets.
21. Corrected Load balance error when using multiple PPPoE connection with the same gateway.


**********************************************************************

    Release Notes for Vigor 2960
    Firmware Version    : 1.0.6 (Formal Release)
    Release Date        : 12th December 2012
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

[Improvements]
1.  Support VPN(IPsec) Routing Acceleration.
2.  Support VPN Alarm via E-mail & Syslog.
3.  Support VPN Graph for Syslog utility.
4.  Support PPPoE server for LAN PC connection.
5.  Add QQ account filter.
6.  Add LDAP/AD for VPN PPTP, L2TP authentication.
7.  URL Content Filter can block HTTPS connection by host keyword.
8.  Improved: WCF (Web Content Filter) supports HTTPS block by web category.

**********************************************************************

    Release Notes for Vigor 3900
    Firmware Version    : 1.0.5 (Formal Release)
    Release Date        : 17th August 2012
    Applicable Models   : Vigor 2960
    Locale              : UK ONLY

**********************************************************************

First Firmware Release

[END OF FILE]